IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-07-28T12:27:13"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130709_2115(x64) - Exporter 3.12.0.0 - Alternate UI 2.12.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "KovacsG_InOptionsGeneralUsername" of Organization (no name given)
  Owner history of Person "KovacsG_InOptionsGeneralUsername" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1469704659 (2016-07-28T11:17:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Westminster, London, UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWSEGMENT | type IFCCABLESEGMENTTYPE "Standard" | object type "Standard" | names: "NBS_CMDLtd_PwrBsbrTrnkng_BetatrakUnderfloorBusbar_1200mm:Standard:232262" | material: "NBS_Concept" | property sets: COBie

Types
  IFCCABLESEGMENTTYPE "Standard" | CABLESEGMENT | 1 occurrence | material: "NBS_Concept" | property sets: NBS_General, NBS_Data, Pset_CableSegmentTypeCableSegment, Pset_BuildingElementProxyCommon, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWSEGMENT)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_60_70_48_07:Busbar trunking feed units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Click-fit underfloor power distribution" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Choice: a comprehensive range of supply systems. Flexibility: can be used in new or existing layouts. Versatility: all kinds of configurations are possible including bends/corners. Safety: colour coded tap offs for easy recognition. Sliding dust covers to protect outlets. Height clearance: low profile busbar suitable for shallow floor voids. Convenience: variety of Betatrak® lengths with different socket centres. 300 mm standard (150 mm and 600 mm available on request)" (IFCTEXT)
    Finish = "Galvanized steel" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@cmd-ltd.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "PBST3312" (IFCTEXT)
    ModelReference = "Betatrak Underfloor Busbar" (IFCTEXT)
    Name = "PowerBusbarTrunking_BetatrakUnderfloorBusbar_1200mm-Standard_CMDLtd" (IFCTEXT)
    NominalWidth = 38. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "1200 x 38 x 75 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CMDLtd_PowerBusbarTrunking_BetatrakUnderfloorBusbar_1200mm-Standard" (IFCTEXT)
    ManufacturerName = "CMD Ltd" (IFCTEXT)
    ManufacturerURL = "www.cmd-ltd.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/svzqfzev" (IFCTEXT)
    NBSDescription = "Power busbar trunking" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "90-50-45/320" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cmd-ltd.com/products/betatrak-busbar" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_60_70_48_07" (IFCTEXT)
    Uniclass2015Title = "Busbar trunking feed units" (IFCTEXT)
    Uniclass2015Version = "Products v1.3" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "n/a" (IFCTEXT)
    AccessoryOptions = "Feed units; tap-off units; flexible corners and kits" (IFCTEXT)
    AdditionalCircuits = "n/a" (IFCTEXT)
    Assembly = "Fully type-tested" (IFCTEXT)
    Attitude = "n/a" (IFCTEXT)
    AttitudeOptions = "Horizontal; Vertical" (IFCTEXT)
    CasingColour = "Steel, metallic" (IFCTEXT)
    CasingFinish = "Self finished" (IFCTEXT)
    CasingIngressProtectionMinimum = "n/a" (IFCTEXT)
    CasingMaterial = "Galvanized steel" (IFCTEXT)
    CasingStandard = "n/a" (IFCTEXT)
    Conductors = "Copper" (IFCTEXT)
    Configuration = "n/a" (IFCTEXT)
    CurrentRating = "63 A" (IFCTEXT)
    EnvironmentalProductDeclaration = "n/a" (IFCTEXT)
    MechanicalDesignAdditionalLoads = "n/a" (IFCTEXT)
    MechanicalDesignMechanicalLoads = "n/a" (IFCTEXT)
    PlaceOfInstallation = "n/a" (IFCTEXT)
    PlaceOfInstallationOptions = "Indoor; Underfloor" (IFCTEXT)
    ProspectiveRatedShortCircuitCurrent1s = "n/a" (IFCTEXT)
    ProtectionAgainstElectricShock = "n/a" (IFCTEXT)
    SocketNumber = 4 (IFCINTEGER)
    Supports = "n/a" (IFCTEXT)
    VoltageRating = "High voltage" (IFCTEXT)
  Pset_CableSegmentTypeCableSegment | properties | on 1 type object
    CableInsulationMaterial = "Flame Retardant Polycarbonate" (IFCTEXT)
    CrossSectionalArea = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    MaxOperatingTemperature = 0. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    NominalHeight = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidthOrDiameter = 38. (IFCLENGTHMEASURE) [MILLI METRE]
    NormalOperatingTemperature = 0. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
    SheathColor = "n/a" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 type object
    Reference = "n/a" (IFCIDENTIFIER)